***RTL FILE of SAP1 Processor Project***

***(Modifed Processor)***

***Group:-*** *G7*

***Team:-***

1. *Ibrahim Samy Section 1*
2. *Yahia Mohammed Section 4*
3. *Yahia Shaban Section 4*
4. *Youssef Samy Section 4*

***Instructions Table:-***

|  |  |  |  |
| --- | --- | --- | --- |
| Instruction | Opcode | Memory Access | Meaning |
| LDA | *000* | *Yes (5-bti address)* | *Load Memory Word to ACC* |
| ADD | *001* | *Yes (5-bti address)* | *Add Memory Word to ACC* |
| SUB | *010* | *Yes (5-bti address)* | *Sub Memory Word from ACC* |
| SHIFT LEFT | *011* | *No* | *Shift the ACC to Left* |
| SHIFT RIGHT | *100* | *No* | *Shift the ACC to Right* |
| OUT | *101* | *No* | *Move the ACC content to Out register* |
| HLT | *111* | *No* | *Stop program execution* |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Instruction | Time Signal | Phase | Micro-Operation | CP  H | EP  H | LM  L | CE  L | LI  L | EI  L | LA  L | EA  H | SU  ALU | EU  H | LB  L | LO  L |
| XXX | *T1* | *Fetch* | *MAR 🡨 PC* | **0** | **1** | **0** | **1** | **1** | **1** | **1** | **0** | **00** | **0** | **1** | **1** |
| *T2* | *Fetch* | *PC 🡨 PC+1*  *IR 🡨 RAM[MAR]* | **1** | **0** | **1** | **0** | **0** | **1** | **1** | **0** | **00** | **0** | **1** | **1** |
| LDA | *T3* | *Execute* | *MAR 🡨 IR(4..0)* | **0** | **0** | **0** | **1** | **1** | **0** | **1** | **0** | **00** | **0** | **1** | **1** |
| *T4* | *Execute* | *A 🡨 RAM[MAR]*  *SC 🡨 0* | **0** | **0** | **1** | **0** | **1** | **1** | **0** | **0** | **00** | **0** | **1** | **1** |
| ADD | *T3* | *Execute* | *MAR 🡨 IR(4..0)* | **0** | **0** | **0** | **1** | **1** | **0** | **1** | **0** | **00** | **0** | **1** | **1** |
| *T4* | *Execute* | *B 🡨 RAM[MAR]* | **0** | **0** | **1** | **0** | **1** | **1** | **1** | **0** | **00** | **0** | **0** | **1** |
| *T5* | *Execute* | *A 🡨 A + B*  *SC 🡨 0* | **0** | **0** | **1** | **1** | **1** | **1** | **0** | **0** | **00** | **1** | **1** | **1** |
| SUB | *T3* | *Execute* | *MAR 🡨 IR(4..0)* | **0** | **0** | **0** | **1** | **1** | **0** | **1** | **0** | **00** | **0** | **1** | **1** |
| *T4* | *Execute* | *B 🡨 RAM[MAR]* | **0** | **0** | **1** | **0** | **1** | **1** | **1** | **0** | **00** | **0** | **0** | **1** |
| *T5* | *Execute* | *A 🡨 A + B’ + 1*  *SC 🡨 0* | **0** | **0** | **1** | **1** | **1** | **1** | **0** | **0** | **11** | **1** | **1** | **1** |
| SHIFT LEFT | *T3* | *Execute* | *A 🡨 SLL A*  *SC 🡨 0* | **0** | **0** | **1** | **1** | **1** | **1** | **0** | **0** | **10** | **1** | **1** | **1** |
| SHIFT RIGHT | *T3* | *Execute* | *A 🡨 SRL A*  *SC 🡨 0* | **0** | **0** | **1** | **1** | **1** | **1** | **0** | **0** | **01** | **1** | **1** | **1** |
| OUT | *T3* | *Execute* | *OUT 🡨A*  *SC 🡨 0* | **0** | **0** | **1** | **1** | **1** | **1** | **1** | **1** | **00** | **0** | **1** | **0** |
| HLT | *T3* | *Execute* | *HALT 🡨 1* | **0** | **0** | **1** | **1** | **1** | **1** | **1** | **0** | **00** | **0** | **1** | **1** |